For 1990-2009 cars

# 3-2 COAST DOWN CLUNK (NEW VALVE BODY SPACER PLATE)

#### SUBJECT: 3-2 COAST DOWN CLUNK (NEW VALVE BODY SPACER PLATE)

#### VEHICLES AFFECTED: 1993 "F" CARS WITH 5.7L (LTI) ENGINE AND 4L60 TRANSMISSION

#### CONDITION:

--------- Some vehicles equipped with a 1993 HYDRA-MATIC 4L60 transmission built before February 8, 1993 (Julian Date 039) may exhibit a 3-2 coast down clunk.

#### CAUSE:

----- A revised 3-2 calibration has been released for the 4L60 transmission.

#### CORRECTION:

---------- To eliminate the 3-2 coast down clunk install a new valve body spacer plate.

Description Part Number ----------- ----------- valve body spacer plate 8686065

#### NOTE: 1993 HYDRA-MATIC 4L60 transmissions built on or after February 8, 1993 (Julian Date 039) have been assembled with a new valve body spacer plate.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.