For 1990-2009 cars

## Front Side Door Window Switch Replacement Chevrolet

### Removal Procedure

Important: Protect the trim panel with a rag when prying up the switch to prevent marring the trim panel.

1. Pry up the rear edge of the driver side switch, the front edge of the passenger side switch.
2. Slide the driver side switch rearward, the passenger side switch forward, out of the door trim panel.
3. Disconnect the electrical connector (5) from the window switches (4).
4. Remove the power window switch (4) from panel.

### Installation Procedure

1. Insert switch assembly into panel.
2. Install the power window switch (4) to the panel.
3. Connect the electrical connector (5) to the switches (4).
4. Insert the front edge of the driver side switch, the rear edge of the passenger side switch, into the door trim panel.
5. Press the rear edge of the driver side switch, the front edge of the passenger side switch, into the trim panel to secure.

## Front Side Door Window Switch Replacement Pontiac

### Removal Procedure

Important: Protect the trim panel with a rag when prying up the switch to prevent marring the trim panel.

1. Pry up the rear of the driver side switch, the front edge of the passenger side switch.
2. Slide the driver side switch rearward, the passenger side switch forward, out of the door trim panel.
3. Disconnect the power window switch electrical connector (4).
4. Remove the power window switches (3) from the panel.

### Installation Procedure

1. Install the power window switches (3) to the panel.
2. Connect the power window switch electrical connector (4).
3. Insert the front edge of the driver side switch, the rear edge of the passenger side switch, into the door trim panel.
4. Press the rear edge of the driver side switch, the front edge of the passenger side switch, into the trim panel to secure.