For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank filler pocket. Refer to Fuel Tank Filler Pipe Housing Replacement .
2. Install the fuel tank filler cap.
3. Drill out the 4 rivets.
4. Remove the fuel tank filler door.

Pry back the sound insulating material around the filler door hinge, as needed.

### Installation Procedure

1. Install the fuel tank filler door.
2. Alternately install the 4 rivets from top to bottom.
3. Remove the fuel tank filler cap.
4. Install the fuel tank filler pocket. Refer to Fuel Tank Filler Pipe Housing Replacement .