For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 41099 Solenoid Socket

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the electrical connector (1) from the reverse lockout solenoid (2).
3. Place a drain pan under the transmission in case any fluid drips out.
4. Remove the reverse lockout solenoid using J 41099 .
5. Remove the reverse lockout assembly bolt.
6. Remove the reverse lockout assembly, if necessary.

### Installation Procedure

#### Tools Required

J 41099 Solenoid Socket

1. Install the reverse lockout assembly, if necessary.
2. Install the reverse lockout assembly bolt.

Tighten
Tighten the reverse lockout assembly bolt to 18 N·m (13 lb ft).

3. Install the reverse lockout solenoid using the J 41099 .

Tighten
Tighten the reverse lockout solenoid to 40 N·m (30 lb ft).

4. Remove the drain pan.
5. Connect the electrical connector (1) to the reverse lockout solenoid (2).
6. Check the transmission fluid level. Refer to Transmission Fluid Level Inspection .
7. Lower the vehicle.