For 1990-2009 cars

1. Remove the oil pump driveshaft bolts.
2. Remove the oil pump driveshaft.
3. Remove the camshaft retainer bolts and retainer.

Important: All camshaft journals are the same diameter, so care must be used in removing the camshaft to avoid damage to the bearings.

4. Remove the camshaft.

4.1. | Install the three 5/16--18 x 4.0 inch bolts in the camshaft front bolt holes.

4.2. | Carefully rotate and pull the camshaft out of the bearings.