For 1990-2009 cars

# LOOSE AND/OR WAVY DOOR GLASS BELT SEALING STRIP

#### SUBJECT: LOOSE AND/OR WAVY DOOR GLASS BELT SEALING STRIP

#### VEHICLES AFFECTED: 1984 - 1988 F CARS

Owner comments of loose and/or wavy door glass belt sealing strip may be addressed without replacing the complete door trim pad assembly.

The upper portion of the trim pad is available from GM Parts, Group # 14.691, P/N 12394510, Right Hand and 12394511, Left Hand. These support assemblies include the sealing strip.

Remove the front door belt support using tool J-28626-A, Kent Moore or equivalent. Install new support using same inverted nuts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.