For 1990-2009 cars

# TWIN LIFT-OFF HATCH ROOF WIND NOISE/WATER LEAK REPAIR

THIS BULLETIN IS DESIGNED TO ASSIST DEALER PERSONAL IN DIAGNOSING AND CORRECTING WATER LEAK AND WIND NOISE COMPLAINTS ON CARS EQUIPPED WITH FISHER BODY TWIN LIFT-OFF HATCH ROOF OPTION... WATER TEST... THE TECHNICIAN PERFORMING THE REPAIRS SHOULD PERSONALLY WATER TEST AND/OR ROAD TEST THE VEHICLE TO DETERMINE THE SOURCE OF THE WATER LEAK, NOISE OR WIND NOISE COMPLAINTS BEFORE BEGINNING REPAIR OPERATIONS. THE TEST RESULTS SHOULD PIN-POINT THE AREA WHERE REPAIRS ARE NEEDED. CHECK WEDGE PLATE CONTACT** BEFORE ADJUSTING THE LIFT-OFF PANEL, THE DOOR TO LOCK PILLAR WEDGE PLATES MUST MAKE CONTACT. TO CHECK WEDGE PLATE CONTACT, APPLY A PIECE OF MASKING TAPE OVER LOCK PILLAR WEDGE PLATE AND CLOSE DOOR. IF THE TAPE IS NOT TORN, ADDITIONAL SHIM(S) ARE REQUIRED AND THE CHECKING PROCEDURE MUST BE PERFORMED AFTER THE SHIMS ARE ADDED. **ALIGNMENT AND ADJUSTMENTS** DOOR GLASS AND FILLER PANEL (SEE PAPER BULLETIN FOR ADDITIONAL DETAIL AND ILLUSTRATIONS)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.