For 1990-2009 cars

### Removal Procedure

1. Remove the plug (5) from the side rail.
2. Use a 13 mm drill bit in order to drill out the damaged nut (2).

### Installation Procedure

1. Place an anti-rotation nut (1) on top of the drilled out nut (2).
2. Align the front crossmember to the side rail.
3. Finger tighten the crossmember bolt (3) and the washer (4).

Tighten
Tighten the lower crossmember bolt to 125 N·m (92 lb ft).

4. Install the plug (5) to the side rail.