For 1990-2009 cars

With the ignition switch in the RUN position, voltage is applied through the TURN B/U Fuse 2 to the backup lamp switch (manual transmission) or the transmission range switch (automatic transmission) through circuit 141. When either transmission is shifted into reverse, voltage is applied through circuit 24 to the backup lamps turning them on provided they have ground circuit 1250.