For 1990-2009 cars

### Removal Procedure

1. Disconnect the rear license lamp electrical connector.
2. Remove the rear license lamp screws.
3. Remove the rear license lamp from the rear bumper fascia.

### Installation Procedure

1. Install the rear license lamp to the rear bumper fascia.
2. Install the rear license lamp screws.

Tighten
Tighten the rear license lamp screws to 1.9 N·m (17 lb in).

3. Connect the rear license lamp electrical connector.