For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Suitably support the vehicle.
2. Remove the exhaust pipe hanger nut from the exhaust muffler hanger.
3. Loosen the muffler clamp.
4. Slide the exhaust pipe out of the muffler.
5. Remove the muffler.

### Installation Procedure

1. Install the muffler.
2. Slide the exhaust pipe into the muffler.
3. Install the muffler clamp.

Tighten
Tighten the muffler clamp to 68 N·m (50 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the exhaust pipe hanger nut.

Tighten
Tighten the exhaust pipe hanger nut to 20 N·m (15 lb ft).

Important: When installing an exhaust muffler, follow clearance specifications for proper alignment.

5. Lower the vehicle.