For 1990-2009 cars

# SEAT SPRING NOISE REPOSITION NYLON SLEEVE

#### SUBJECT: SEAT SPRING N.01SE (REPOSITION NYLON SLEEVE)

VEHICLES AFFECTED: 1993 "F" MODEL

#### APPLICATION:

1993 Chevrolet and Pontiac F-Car

#### CONDITION:

Seat spring noise from passenger front seat.

#### CAUSE:

Nylon sleeve on seat adjuster return spring positioned too far forward.

#### CORRECTION:

Reposition nylon sleeve on return spring.

1. Move passenger seat forward.

2. From the rear, reach under seat and disconnect retum spring from front of outboard adjuster then from rear.

3. Position rear end of spring wire through second row of nylon sleeve webbing and slide sleeve forward over spring. (See Illustration.)

4. Reinstall spring to outboard adjuster.

For vehicles repaired under warranty use:

Labour Time: 0.2 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.