For 1990-2009 cars

Table 1: | A/C Compressor Clutch
Table 2: | A/C Refrigerant Pressure Sensor
Table 3: | Camshaft Position (CMP) Sensor
Table 4: | Crankshaft Position (CKP) Sensor
Table 5: | Data Link Connector (DLC)
Table 6: | Engine Coolant Temperature Sensor
Table 7: | Engine Oil Level Switch
Table 8: | Evaporative Emission (EVAP) Canister Purge Valve
Table 9: | Evaporative Emission (EVAP) Canister Vent Valve
Table 10: | Exhaust Gas Recirculation (EGR) Valve
Table 11: | Fuel Injector #1
Table 12: | Fuel Injector #3
Table 13: | Fuel Injector #5
Table 14: | Fuel Injector #2
Table 15: | Fuel Injector #4
Table 16: | Fuel Injector #6
Table 17: | Fuel Tank Pressure Sensor
Table 18: | Heated Oxygen Sensor (HO2S), Bank 1, Sensor 1
Table 19: | Heated Oxygen Sensor (HO2S), Bank 2, Sensor 1
Table 20: | Heated Oxygen Sensor (HO2S), Bank 1, Sensor 3
Table 21: | Idle Air Control (IAC) Valve
Table 22: | Intake Air Temperature (IAT) Sensor
Table 23: | Manifold Absolute Pressure (MAP) Sensor
Table 24: | Mass Air Flow (MAF) Sensor
Table 25: | Throttle Position (TP) Sensor
Table 26: | Vehicle Speed Sensor (VSS)

#### A/C Compressor Clutch

Connector Part Information |

• | 1216-2017

• | 2 Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 59 | A/C Compressor Clutch Control
B | BLK | 450 | A/C Compressor Clutch Ground

#### A/C Refrigerant Pressure Sensor

Connector Part Information |

• | 1211-0192

• | 3 Way M Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 720 | A/C Refrigerant Pressure Sensor Ground
B | LT BLU/BLK | 1688 | A/C Refrigerant Pressure Sensor 5.0V Reference
C | BLK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 1216-2279

• | 3 Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | Camshaft Position (CMP) Sensor Signal - Input
B | RED/BLK | 645 | Reference Low
C | WHT/BLK | 644 | Ignition Feed

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162834

• | 4 Way Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU/WHT | 1800 | Crankshaft Position (CKP) Sensor Signal - Input
B | YEL | 573 | Reference Low
C | RED/BLK | 645 | Ignition Feed
D | WHT/BLK | 644 | Ignition Feed

#### Data Link Connector (DLC)

Connector Part Information |

• | 1211-0250

• | 16 Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PPL | 1807 | Serial Data Line-Class 2
3 | -- | -- | Not Used
4 | BLK | 350 | Ground
5 | BLK/WHT | 351 | Ground
6 | -- | -- | Not Used
7 | -- | -- | Not Used
8 | BLK/WHT | 1455 | Keyless Entry Program Enable Signal
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | DK GRN | 835 | Serial Data Line - Entertainment and Comfort (EC)
15 | -- | -- | Not Used
16 | ORN | 1140 | Fuse Output Battery

#### Engine Coolant Temperature Sensor

Connector Part Information |

• | 1211-0192

• | 3 Way F Metri-Pack 150 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 718 | Engine Coolant Temperature (ECT) Sensor Ground
B | YEL | 410 | Engine Coolant Temperature (ECT) Sensor Signal
C | DK BLU | 135 | Engine Coolant Temperature (ECT) Sensor Output

#### Engine Oil Level Switch

Connector Part Information |

• | 1205-2641

• | 2 Way F Metri-Pack 150 Series Sealed

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 451 | Ground
B | BRN | 1174 | Oil Level Switch Signal

#### Evaporative Emission (EVAP) Canister Purge Valve

Connector Part Information |

• | 1205-2643

• | 2 Way Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition Feed
B | WHT | 1310 | EVAP Canister Purge Valve Control

#### Evaporative Emission (EVAP) Canister Vent Valve

Connector Part Information |

• | 1205-2643

• | 2 Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition Feed
B | WHT | 1310 | EVAP Canister Vent Valve Control

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 1218-6056

• | 5 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | Exhaust Gas Recirculation (EGR) Valve Control
B | BLK | 552 | Exhaust Gas Recirculation (EGR) Sensor Ground
C | BRN | 1456 | Exhaust Gas Recirculation (EGR) Pintle Position
D | GRY | 598 | Exhaust Gas Recirculation (EGR) 5V Reference
E | LT BLU | 697 | Exhaust Gas Recirculation (EGR) Valve Ignition Feed

#### Fuel Injector #1

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | BLK | 1744 | Fuel Injector #1 Control

#### Fuel Injector #3

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | PNK/BLK | 1746 | Fuel Injector #3 Control

#### Fuel Injector #5

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | BLK/WHT | 845 | Fuel Injector #5 Control

#### Fuel Injector #2

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | LT GRN/BLK | 1745 | Fuel Injector #2 Control

#### Fuel Injector #4

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | LT BLU/BLK | 844 | Fuel Injector #4 Control

#### Fuel Injector #6

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition (RUN and START)
B | YEL/BLK | 846 | Fuel Injector #6 Control

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Fuel Sensor Ground
B | DK GRN | 890 | Fuel Tank Pressure Signal
C | GRY | 416 | 5V Sensor Feed

#### Heated Oxygen Sensor (HO2S), Bank 1, Sensor 1

Connector Part Information |

• | 1216-0482

• | 4 Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN /WHT | 1653 | LF Heated Oxygen Sensor (HO2S) - Low
B | PPL/WHT | 1665 | LF Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S), Bank 2, Sensor 1

Connector Part Information |

• | 1216-0482

• | 4 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1667 | RF Heated Oxygen Sensor (HO2S) - Low
B | PPL | 1666 | RF Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S), Bank 1, Sensor 3

Connector Part Information |

• | 121-60825

• | 4 Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 1981 | Heated Oxygen Sensor (HO2S) - Low
B | DK BLU | 1980 | Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 1216-2190

• | 4 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | Idle Air Control (IAC) Valve Coil B Signal - Low
B | LT GRN WHT | 1749 | Idle Air Control (IAC) Valve Coil B Signal - High
C | LT BLU/BLK | 1748 | Idle Air Control (IAC) Valve Coil A Signal - Low
D | LT BLU/WHT | 1747 | Idle Air Control (IAC) Valve Coil A Signal - High

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 1216-2199

• | 2 Way F Metri-Pack 150.2 Series Pull to Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 719 | Intake Air Temperature (IAT) Sensor Ground
B | TAN | 472 | Intake Air Temperature (IAT) Sensor Signal

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 1212-9946

• | 3 Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Manifold Absolute Pressure (MAP) Sensor Ground
B | LT GRN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | GRY | 598 | Manifold Absolute Pressure (MAP) Sensor 5.0V Reference

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | Mass Air Flow (MAF) Sensor Signal
B | BLK/WHT | 451 | Ground
C | PNK | 539 | Ignition Feed

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 1211-0293

• | 3 Way F Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 452 | Sensor Ground
B | DK BLU | 417 | Throttle Position Sensor Signal
C | GRY | 598 | Throttle Position (TP) Sensor 5V Reference

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 1216-2195

• | 2 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | Vehicle Speed Sensor (VSS) Signal - Low
B | YEL | 400 | Vehicle Speed Sensor (VSS) Signal - High