For 1990-2009 cars

## Windshield Side Garnish Molding Replacement Without Lift Off Window Pan

### Removal Procedure

1. Open the vehicle door.
2. Remove the windshield upper garnish molding by pulling away from the inner side frame.

### Installation Procedure

1. Install the windshield upper garnish molding.

• | Align tabs on garnish molding to holes in inner side frame and apply pressure to secure.

• | Align S-clips on garnish molding to door opening flange and apply pressure to secure.

2. Close the vehicle door.

## Windshield Side Garnish Molding Replacement With Lift Off Window Pan

### Removal Procedure

1. Open the vehicle door.
2. Remove the lift-off window panel.
3. Remove the garnish molding screws.
4. Remove the windshield upper garnish molding by pulling away from the inner side frame.

### Installation Procedure

1. Install the upper garnish molding.

• | Align the clips to the holes on the inner side frame and apply pressure to secure.

• | Align S-clips on upper garnish molding to door opening flange and apply pressure to secure.

2. Install the garnish molding screws.

Tighten
Tighten the garnish molding screws to 1.7 N·m (15 lb in).

3. Install the lift-off window panel.
4. Close the vehicle door.