For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Travel (see note) | 51-89 mm | 2.0-3.5 in
Brake Pipe Clearance (Minimum)

- Moving Components

19 mm

0.75 in

- Vibrating Components

13 mm

0.50 in

Hydraulic Brake (Glycol) Fluid | GM P/N 1052535 or equivalent DOT-3 fluid
Note: Brake pedal travel maximum with 445 N (100 lb) of force applied to the pedal with the engine running at idle.