For 1990-2009 cars

# HATCHBACK CLOSING EFFORT WAYS TO REDUCE EFFORT

#### VEHICLES AFFECTED: 1982-1984 Camaro and Firebirds

The 1982-1984 'F' model hatchbacks are designed to provide more cargo space than is available in a standard passenger car while still providing all the same ride and comfort features.

To ensure adequate sealing, this design may require a greater closing effort than some owners expect due to the large volume of air being displaced. Owners should be advised that slightly opening a door or window will significantly reduce the effort required to close the hatch.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.