For 1990-2009 cars

### Removal Procedure

Important: The adjuster assembly cables must always be adjusted each time the adjuster assembly is removed and/or replaced to ensure optimum system performance. Refer to Cable Adjustment .

1. Remove the adjuster assembly splash cover.
2. Remove the cable cam cover.
3. Disconnect the adjuster assembly electrical connector.
4. Remove the nuts attaching the adjuster assembly to the bracket.
5. Remove the cables from the adjuster assembly.

### Installation Procedure

1. Install the cables to the adjuster assembly.
2. Install the adjuster assembly to the mounting bracket (3).
3. Install the adjuster assembly attaching nuts.

Tighten
Tighten the adjuster assembly attaching nuts to 25 N·m (18 lb ft).

4. Connect the adjuster assembly electrical connector.
5. Adjust the adjuster assembly cables. Refer to Cable Adjustment
6. Install the cable cam cover.
7. Install the adjuster assembly splash cover.