For 1990-2009 cars

## Wheel Speed Sensor Jumper Harness Replacement Rear with Traction Control

### Removal Procedure

1. Remove the wheel speed sensor connectors (2,3).
2. Remove the jumper harness grommet from the retainer.
3. Remove the upper jumper harness connector from the rear body pass-thru connector.

### Installation Procedure

1. Install the upper jumper harness connector from the rear body pass-thru connector.
2. Install the jumper harness grommet to the retainer.
3. Install the wheel speed sensor connectors (2,3).

## Wheel Speed Sensor Jumper Harness Replacement Rear without Traction Control

### Removal Procedure

1. Remove the wheel speed sensor connector.
2. Remove the rear wheel speed sensor jumper harness grommet from retainer (1).
3. Remove the upper harness connector from rear body pass-thru connector.

### Installation Procedure

1. Install the upper harness connector from rear body pass-thru connector.
2. Install the rear wheel speed sensor jumper harness grommet from retainer (1).
3. Install the wheel speed sensor connector.

## Wheel Speed Sensor Jumper Harness Replacement Front Left

### Removal Procedure

1. Remove the wheel speed sensor connector.
2. Remove the jumper harness from the retaining clip.
3. Remove the grommet retainer at the inner fender.
4. Remove the transmission cable retainer and various harnesses from restraints at left strut tower to access jumper harness connector.
5. Remove the upper jumper harness connector.
6. Pull the grommet through inner fender pass-thru and remove jumper harness.

### Installation Procedure

1. Route the new jumper harness through inner fender pass-thru.
2. Install the upper jumper harness connector.
3. Install the transmission cable retainer and various harnesses to restraints that may have been disconnected to access jumper harness.
4. Install the grommet retainer at the inner fender.
5. Install the jumper harness from the retaining clip.
6. Install the wheel speed sensor connector.

## Wheel Speed Sensor Jumper Harness Replacement Front Right

### Removal Procedure

1. Remove the wheel speed sensor connector.
2. Remove the jumper harness from the retaining clip.
3. Remove the grommet retainer at the inner fender.
4. Remove the harness cover from the right strut tower.
5. Remove the upper jumper harness connector.
6. Pull the grommet through inner fender pass-thru and remove jumper harness.

### Installation Procedure

1. Route the new jumper harness through inner fender pass-thru.
2. Install the upper jumper harness connector.
3. Install the harness cover on the right strut tower.
4. Install the grommet retainer at the inner fender.
5. Install the jumper harness from the retaining clip.
6. Install the wheel speed sensor connector.