For 1990-2009 cars

Table 1: | In-Line Connector C100
Table 2: | In-Line Connector C101
Table 3: | In-Line Connector C105
Table 4: | In-Line Connector C108
Table 5: | In-Line Connector C120
Table 6: | In-Line Connector C130
Table 7: | In-Line Connector C200A/C200D
Table 8: | In-Line Connector C200B/C200D
Table 9: | In-Line Connector C200C/C200D
Table 10: | In-Line Connector C210
Table 11: | In-Line Connector C211 (Traction Control Module)
Table 12: | In-Line Connector C212
Table 13: | In-Line Connector C220
Table 14: | In-Line Connector C230
Table 15: | In-Line Connector C240
Table 16: | In-Line to Power Seat Switch (LH) C300
Table 17: | In-Line to I/P C310
Table 18: | In-Line Connector C400
Table 19: | In-Line Connector C405A/C405B
Table 20: | In-Line Connector C405C/C405B
Table 21: | In-Line Connector C405D/C405B

#### In-Line Connector C100

Connector Part Information |

• | 12065425

• | 10-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12048253

• | 10 - Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | PNK | 639 | Power feed from injector fuse 9 | A | PNK | 639 | Power feed from injector fuse 9
B | GRN/WHT | 459 | A/C compressor relay control | B | GRN/WHT | 459 | A/C compressor relay control
C | DK GRN | 59 | A/C compressor clutch solenoid feed | C | DK GRN | 59 | A/C compressor clutch solenoid feed
D | GRY | 596 | Reference voltage feed - 5 volt reference (V8 VIN G) | D | GRY | 596 | Reference voltage feed - 5 volt reference (V8 VIN G)
E | DK BLU | 417 | Throttle position sensor signal (V8 VIN G) | E | DK BLU | 417 | Throttle position sensor signal (V8 VIN G)
F | -- | -- | Not Used | F | -- | -- | Not Used
G | PNK | 239 | Power feed from ignition fuse (OBD II) | G | PNK | 239 | Power feed from ignition fuse (OBD II)
H | DK BLU | 473 | Coolant fan relay control | H | DK BLU | 473 | Coolant fan relay control
J | DK GRN | 335 | Coolant fan relay control | J | DK GRN | 235 | Coolant fan relay control
K | BLK | 452 | Sensor return (V8 VIN G) | K | BLK | 452 | Sensor return (V8 VIN G)

#### In-Line Connector C101

Connector Part Information |

• | 12065426

• | 10-Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12065648

• | 10-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | YEL/BLK | 625 | Vehicle anti-theft system starter enable relay output-coil | A | YEL/BLK | 625 | Vehicle anti-theft system starter enable relay output-coil
B | PNK | 839 | Fuse output-ignition 1-type III fuse (V8 VIN G) | B | PNK | 839 | Fuse output-ignition 1-type III fuse (V8 VIN G)
C | BRN | 436 | Air pump relay control | C | BRN | 436 | Air pump relay control
D | GRN/WHT | 465 | Fuel pump relay control | D | GRN/WHT | 465 | Fuel pump relay control
E | PNK | 439 | Fuse output-ignition 1-type III fuse | E | PNK/BLK |  | Fuse output-ignition 1-type III fuse
F | -- | -- | Not Used | F | -- | -- | Not Used
G | ORN | 340 | Fuse output-battery-type III fuse | G | ORN | 340 | Fuse output-battery-type III fuse
H | BLK/WHT | 451 | Ground | H | BLK/WHT | 451 | Ground
J | -- | -- | Not Used | I | -- | -- | Not Used
K | GRY/BLK | 1687 | Ignition retard signal (V8 VIN G) | K | GRY/BLK | 1687 | Ignition retard signal (V8 VIN G)

#### In-Line Connector C105

Connector Part Information |

• | 12047937

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12052454

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | PPL/WHT | 1572 | Traction control system indicator lamp output-failure | A | PPL/WHT | 1572 | Traction control system indicator lamp output-failure
B | PNK | 539 | Fuse output-ignition 1--type III fuse | B | PNK | 539 | Fuse output-ignition --type III fuse1
C | BRN/WHT | 1571 | Traction control system switch signal | C | BRN/WHT | 1571 | Traction control system switch signal
D | DK GRN | 83 | Cruise control signal-disengage (V6 VIN K) | D | DK GRN | 83 | Cruise control signal-disengage (V6 VIN K)
E | TAN | 800 | Serial data signal | E | TAN | 800 | Serial data signal
F | WHT | 85 | Cruise control indicator lamp output (V6 VIN K) | F | WHT | 85 | Cruise control indicator lamp output (V6 VIN K)
G | WHT | 121 | Tachometer signal | G | WHT | 121 | Tachometer signal
H | PPL | 421 | Air injection reaction solenoid relay output-coil | H | PPL | 421 | Air injection reaction solenoid relay output-coil

#### In-Line Connector C108

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12052844

• | 3-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN/WHT | 633 | Camshaft position sensor signal (V8 VIN G) | A | BRN/WHT | 633 | Camshaft position sensor signal (V8 VIN G)
B | PNK/BLK | 632 | Camshaft position sensor return (V8 VIN G) | B | PNK/BLK | 632 | Camshaft position sensor return (V8 VIN G)
C | RED | 631 | Camshaft sensor feed-12 volt reference (V8 VIN G) | C | RED | 631 | Camshaft sensor feed-12 volt reference (V8 VIN G)

#### In-Line Connector C120

Connector Part Information |

• | 12162343

• | 2-Way F Metri-Pack 150 Series

Connector Part Information

• | 12052644

• | 2-Way M Metri-Pack 150 Series

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | YEL | 873 | Wheel speed sensor return-left front | A | YEL | 873 | Wheel speed sensor return-left front
B | LT BLU | 830 | Wheel speed sensor signal-left front | B | LT BLU | 830 | Wheel speed sensor signal-left front

#### In-Line Connector C130

Connector Part Information |

• | 12162343

• | 2-Way F Metri-Pack 150 Series

Connector Part Information

• | 12052644

• | 2-Way M Metri-Pack 150 Series

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | TAN | 833 | Wheel speed sensor return-right front | A | TAN | 833 | Wheel speed sensor return-right front
B | DK GRN | 872 | Wheel speed sensor signal-right front | B | DK GRN | 872 | Wheel speed sensor signal-right front

#### In-Line Connector C200A/C200D

Connector Part Information |

• | 12047842

• | 17-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | DK GRN/WHT | 817 | Vehicle speed signal-4000 pulses per mile | A1 | DK GRN/WHT | 817 | Vehicle speed signal-4000 pulses per mile
A2 | LT BLU | 14 | Turn signal lamp-feed-left front | A2 | LT BLU | 14 | Turn signal lamp-feed-left front
A3 | LT GRN | 867 | ABS failure indicator lamp output | A3 | LT GRN | 867 | ABS failure indicator lamp output
A4 | LT BLU | 20 | Stoplamp feed | A4 | LT BLU | 20 | Stoplamp feed
A5 | YEL/BLK | 1471 | Brake warning indicator lamp feed--secondary | A5 | YEL/BLK | 1471 | Brake warning indicator lamp feed--secondary
A6 | DK GRN | 1433 | Clutch start switch output | A6 | DK GRN | 1433 | Clutch start switch output
A7 | BLK | 28 | Horn relay output-coil | A7 | BLK | 28 | Horn relay output-coil
A8 | GRY | 120 | Fuel pump motor feed | A8 | GRY | 120 | Fuel pump motor feed
A9 | DK BLU | 1537 | ABS indicator lamp output | A9 | DK BLU | 1537 | ABS indicator lamp output
A10 | BRN | 882 | Wheel speed sensor signal-right rear | A10 | BRN | 882 | Wheel speed sensor signal-right rear
A11 | WHT | 883 | Wheel speed sensor return-right rear | A11 | WHT | 883 | Wheel speed sensor return-right rear
A12 | TAN | 800 | Serial data signal-uart 8192 baud--primary | A12 | TAN | 800 | Serial data signal-uart 8192 baud--primary
A13 | BRN/WHT | 1571 | Traction control system switch signal | A13 | BRN/WHT | 1571 | Traction control system switch signal
A14 | RED | 885 | Wheel speed sensor return-left rear | A14 | RED | 885 | Wheel speed sensor return-left rear
A15 | BLK | 884 | Wheel speed sensor signal-left rear | A15 | BLK | 884 | Wheel speed sensor return-left rear
A16 | YEL | 317 | Fog lamp relay feed-coil | A16 | YEL | 317 | Fog lamp relay feed-coil
A17 | YEL/BLK | 68 | Low coolant level indicator lamp output | A17 | YEL/BLK | 68 | Low coolant level indicator lamp output

#### In-Line Connector C200B/C200D

Connector Part Information |

• | 12162504

• | 18-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
B1 | PNK | 3 | Ignition switch output--ignition 1 | B1 | PNK | 3 | Ignition switch output--ignition 1
B2 | TAN/WHT | 33 | Brake warning indicator lamp output | B2 | TAN/WHT | 33 | Brake warning indicator lamp output
B3 | PPL | 34 | Fog lamp feed | B3 | PPL | 34 | Fog lamp feed
B4 | RED | 1302 | Fuse output battery--type 1 fuse | B4 | RED | 1302 | Fuse output battery--type 1 fuse
B5 | YEL | 10 | Headlamp switch output | B5 | YEL | 10 | Headlamp switch output
B6 | RED | 702 | Fuse output-battery--type 1 fuse | B6 | RED | 702 | Fuse output-battery--type 1 fuse
C1 | RED | 102 | Fuse output-battery--type 1 fuse | C1 | RED | 102 | Fuse output-battery--type 1 fuse
C2 | RED | 1002 | Fuse output-battery--type 1 fuse | C2 | RED | 1002 | Fuse output-battery--type 1 fuse
C3 | LT GRN | 11 | High beam headlamp feed | C3 | LT GRN | 11 | High beam headlamp feed
C4 | PPL/WHT | 1572 | Traction control system indicator lamp output-failure | C4 | PPL/WHT | 1572 | Traction control system indicator lamp output-failure
C5 | PPL/WHT | 1035 | Not Used | C5 | PPL/WHT | 1035 | Not Used
C6 | BRN | 4 | Ignition switch output-accessory | C6 | BRN | 4 | Ignition switch output-accessory
D1 | RED | 1202 | Fuse output-battery--type 1 fuse | D1 | RED | 1202 | Fuse output-battery--type 1 fuse
D2 | PNK | 239 | Fuse output-ignition 1--type 111 fuse | D2 | PNK | 239 | Fuse output-ignition 1--type 111 fuse
D3 | YEL | 143 | Fuse output-accessory--type 111 fuse | D3 | YEL | 143 | Fuse output-accessory--type 111 fuse
D4 | BRN | 9 | Park lamp feed | D4 | BRN | 9 | Park lamp feed
D5 | PPL/WHT | 1572 | Traction control system indicator lamp output-failure | D5 | PPL/WHT | 1572 | Traction control system indicator lamp output-failure
D6 | DK BLU | 15 | Turn signal lamp feed-right front | D6 | DK BLU | 15 | Turn signal lamp feed-right front

#### In-Line Connector C200C/C200D

Connector Part Information |

• | 12047840

• | 13-Way F Metri-Pack 280 Series (GRY)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
E1-E2 | -- | -- | Not used | E1-E2 | -- | -- | Not used
E3 | DK BLU/WHT | 149 | Courtesy lamp feed | E3 | DK BLU/WHT | 149 | Courtesy lamp feed
E4 | GRY/BLK | 745 | Door ajar switch signal-left front | E4 | GRY/BLK | 745 | Door ajar switch signal-left front
E5 | BLK/WHT | 746 | Door ajar switch signal-right front | E5 | BLK/WHT | 746 | Door ajar switch signal-right front
E6 | -- | -- | Not used | E6 | -- | -- | Not used
E7 | GRY | 8 | Instrument panel lamp feed | E7 | GRY | 8 | Instrument panel lamp feed
E8 | -- | -- | Not used | E8 | -- | -- | Not used
E9 | ORN | 640 | Fuse output-battery--type 111 fuse | E9 | ORN | 640 | Fuse output-battery--type 111 fuse
E10 | WHT | 156 | Courtesy lamp output | E10 | WHT | 156 | Courtesy lamp output
E11 | BRN | 341 | Fuse output-ignition--type 111 fuse | E11 | BRN | 341 | Fuse output-ignition--type 111 fuse
E12-E13 | -- | -- | Not used | E12-E13 | -- | -- | Not used

#### In-Line Connector C210

Connector Part Information |

• | 1206-5398

• | 8-Way F Metri-Pack 150 Series (Neutral)

Connector Part Information

• | 1206-5396

• | 8-Way M Metri-Pack 150 Series (Neutral)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GRY | 598 | Reference voltage feed--5 volt reference | A | GRY | 598 | Reference voltage feed--5 volt reference
B | WHT | 1310 | Cannister vent valve solenoid output | B | WHT | 1310 | Cannister vent valve solenoid output
C | GRY | 720 | Sensor return | C | GRY | 720 | Sensor return
D | -- | -- | Not Used | D | -- | -- | Not Used
E | DK BLU | 1936 | Fuel gauge sensor signal | E | DK Blue | 1936 | Fuel gauge sensor signal
F | DK GRN | 890 | Fuel tank pressure sensor signal | F | DK GRN | 890 | Fuel tank pressure sensor signal
G | -- | -- | Not Used | G | -- | -- | Not Used
H | PPL | 30 | Fuel Gauge Sensor Signal | H | PPL | 30 | Fuel Gauge Sensor Signal

#### In-Line Connector C211 (Traction Control Module)

Connector Part Information |

• | 12077777

• | 8-Way M Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064766

• | 8-Way F Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | DK BLU | 417 | Throttle position sensor signal | A | DK BLU | 417 | Throttle position sensor signal
B | WHT | 560 | Throttle relaxer motor feed | B | WHT | 560 | Throttle relaxer motor feed
C | ORN | 1540 | Fuse output-battery--type III fuse | C | ORN | 1540 | Fuse output-battery--type III fuse
D | GRY | 561 | Throttle relaxer motor return | D | GRY | 561 | Throttle relaxer motor return
E | BLK/WHT | 151 | Ground | E | BLK/WHT | 151 | Ground
F-H | -- | -- | Not used | F-H | -- | -- | Not used

#### In-Line Connector C212

Connector Part Information |

• | 12064769

• | 10-Way F Metri- Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064769

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | ORN/BLK | 463 | Traction control system signal-torque desired | A | ORN/BLK | 463 | Traction control system signal-torque desired
B | PNK | 739 | Fuse output-ignition--type III fuse | B | PNK | 739 | Fuse output-ignition--type III fuse
C | TAN/BLK | 464 | Traction control system signal torque delivered | C | TAN/BLK | 464 | Traction control system signal torque delivered
D | WHT | 560 | Throttle relaxer motor feed | D | WHT | 560 | Throttle relaxer motor feed
E | ORN | 1540 | Fuse output-battery--type III fuse | E | ORN | 1540 | Fuse output-battery--type III fuse
F | GRY | 561 | Throttle relaxer motor return | F | GRY | 561 | Throttle relaxer motor return
G | BLK/WHT | 151 | Ground | G | BLK/WHT | 151 | Ground
H | -- | -- | Not used | H | -- | -- | Not used
J | BLK | 452 | Sensor return | J | BLK | 452 | Sensor return
K | GRY | 596 | Reference voltage feed-5 volt reference | K | GRY | 596 | Reference voltage feed-5 volt reference

#### In-Line Connector C220

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | RED | 225 | Generator feed to instrument cluster | A | RED | 225 | Generator feed to instrument cluster
B | TAN | 31 | Oil pressure feed to instrument cluster | B | TAN | 31 | Oil pressure feed to instrument cluster
C | BRN/WHT | 1173 | Low oil level indicator lamp output | C | BRN/WHT | 1173 | Low oil level indicator lamp output
D | -- | -- | Not Used | D | -- | -- | Not Used
E | -- | -- | Not Used | E | -- | -- | Not Used
F | BLK/WHT | 451 |  | F | 451 |  |
G | GRN/WHT | 817 | Vehicle speed signal | G | GRN/WHT | 817 | Vehicle speed signal
H | WHT | 375 | Skip shift indicator control (V8 VIN G Manual transmission) | H | WHT | 375 | Skip shift indicator control (V8 VIN G Manual transmission)
J | YEL/BLK | 625 | Vehicle anti-theft system starter enable relay output--coil | J | YEL/BLK | 625 | Vehicle anti-theft system starter enable relay output--coil
K | DK GRN | 135 | Coolant temperature feed to instrument cluster | K | DK GRN | 135 | Coolant temperature feed to instrument cluster

#### In-Line Connector C230

Connector Part Information |

• | 12064871

• | 10-Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064872

• | 10-Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GRY | 48 | Clutch anticipate signal (V6 VIN K Only | A | GRY | 48 | Clutch anticipate signal (V6 VIN K Only
B | BRN/WHT | 419 | Service Engine Soon indicator feed | B | BRN/WHT | 419 | Service Engine Soon indicator feed
C | -- | -- | Not Used | C | -- | -- | Not Used
D | WHT | 121 | Tachometer signal to instrument cluster | D | WHT | 121 | Tachometer signal to instrument cluster
E | DK BLU | 229 | Theft deterrent-fuel enable feed | E | DK BLU | 229 | Theft deterrent-fuel enable feed
F | DK GRN/WHT | 762 | A/C request signal | F | DK GRN/WHT | 762 | A/C request signal
G | PNK | 539 | Brake pedal switch output--torque convertor clutch (V6 VIN K Auto Trans) | G | PNK | 539 | Brake pedal switch output--torque convertor clutch (V6 VIN K Auto Trans)
G | BRN | 141 | Fuse output-ignition 3-type III fuse (V6 VIN K MAN TRANS) | G | BRN | 141 | Fuse output-ignition 3-type III fuse (V6 VIN K MAN TRANS)
H | PPL | 420 | (Automatic) TCC switch power feed | H | PPL | 420 | (Automatic) TCC switch power feed
J | ORN/BLK | 434 | (Automatic) Park/Neutral feed from transmission range switch | J | ORN/BLK | 434 | (Automatic) Park/Neutral feed from transmission range switch
J | LT GRN | 24 | Back-up lamp feed (V6 VIN K Manual transmission) | J | LT GRN | 24 | Back-up lamp feed (V6 VIN K Manual transmission)
K | PPL | 1807 | Output field service enable | K | PPL | 1807 | Output field service enable

#### In-Line Connector C240

Connector Part Information |

• | 12045688

• | 6-Way M Metri-Pack Series 280 (BLK)

Connector Part Information

• | 12047886

• | 6-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 1856 | Speaker feed-left front-tweeter (UZ7) | A | BLK | 1856 | Speaker feed-left front-tweeter (UZ7)
A | DK BLU | 1857 | Speaker feed-left front-midrange (W54 W55) | A | DK BLU | 1857 | Speaker feed-left front-midrange (W54 W55)
B | DK BLU | 1857 | Speaker feed-left front-midrange (UZ7) | B | DK BLU | 1857 | Speaker feed-left front-midrange (UZ7)
B | TAN | 201 | Speaker feed-left front (W54 W55) | B | TAN | 201 | Speaker feed-left front (W54 W55)
C | LT BLU | 1957 | Speaker return-left front-midrange (UZ7) | C | LT BLU | 1957 | Speaker return-left front-midrange (UZ7)
C | GRY | 118 | Speaker return-left front (W54 W55) | C | GRY | 118 | Speaker return-left front (W54 W55)
D | YEL | 1956 | Speaker return--left front tweeter (UZ7) | D | YEL | 1956 | Speaker return--left front tweeter (UZ7)
D | LT BLU | 1957 | Speaker feed-left front-midrange (W54 W55) | D | LT BLU | 1957 | Speaker feed-left front-midrange (W54 W55)
E | PPL | 1952 | Speaker return--right front tweeter (UZ7) | E | PPL | 1952 | Speaker return--right front tweeter (UZ7)
E | ORN | 1853 | Speaker feed-right front-midrange (W54 W55) | E | ORN | 1853 | Speaker feed-right front-midrange (W54 W55)
F | DK GRN | 1953 | Speaker return-right front-midrange (UZ7) | F | DK GRN | 1953 | Speaker return-right front-midrange (UZ7)
F | DK GRN | 117 | Speaker return-right front (W54 W55) | F | DK GRN | 117 | Speaker return-right front (W54 W55)
G | ORN | 1853 | Speeker feed-right front-tweeter (UZ7) | G | ORN | 1853 | Speeker feed-right front-tweeter (UZ7)
G | LT GRN | 200 | Speaker feed-right front (W54 W55) | G | LT GRN | 200 | Speaker feed-right front (W54 W55)
H | Lt GRN | 1852 | Speaker feed--right front--tweeter (UZ7) | H | Lt GRN | 1852 | Speaker feed--right front--tweeter (UZ7)
H | DK GRN | 1953 | Speaker return-right front midrange (W54 W55) | H | DK GRN | 1953 | Speaker return-right front midrange (W54 W55)

#### In-Line to Power Seat Switch (LH) C300

Connector Part Information |

• | 12064752

• | 6-Way Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 764 | Pneumatic seat relay feed-coil-drive deflate
B | WHT | 766 | Pneumatic seat relay feed-coil-drive inflate
C | ORN | 1240 | Fuse output-battery
D | BLK | 1450 | Ground
E | BRN | 763 | Pneumatic seat solenoid feed-lumbar-driver
F | PPL | 765 | Pneumatic seat solenoid feed-lateral-driver

#### In-Line to I/P C310

Connector Part Information |

• | 12015199

• | 2-Way Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1240 | Fuse output-battery
B | BLK | 1450 | Ground

#### In-Line Connector C400

Connector Part Information |

• | 12065781

• | 6-Way M Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064762

• | 6-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | LT BLU | 20 | Stop lamp feed | A | LT BLU | 20 | Stop lamp feed
B | -- | -- | Not used | B | -- | -- | Not used
C | BRN | 9 | Park lamp feed | C | BRN | 9 | Park lamp feed
D | YEL | 18 | Stop/trun lamp feed-left rear | D | YEL | 18 | Stop/trun lamp feed-left rear
E | DK GRN | 19 | Stop/turn lamp feed-left rear | E | DK GRN | 19 | Stop/turn lamp feed-left rear
F | LT GRN | 24 | Back-up lamp feed | F | LT GRN | 24 | Back-up lamp feed

#### In-Line Connector C405A/C405B

Connector Part Information |

• | 12146442

• | 7-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12160830

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
3A | PPL | 30 | Fuel gauge sensor signal | 3A | PPL | 30 | Fuel gauge sensor signal
3B | GRY | 120 | Fuel pump motor feed | 3B | GRY | 120 | Fuel pump motor feed
3C | BLK | 150 | Ground | 3C | BLK | 150 | Ground
3D | GRY/BLK | 416 | Reference voltage feed-5 volt reference | 3D | GRY/BLK | 598 | Reference voltage feed-5 volt reference
3E | -- | -- | Not used | 3E | -- | -- | Not used
3F | BLK/WHT | 651 | Fuel gauge sensor ground | 3F | BLK/WHT | 720 | Fuel gauge sensor ground
3G | ORN/BLK | 469 | Fuel Tank pressure sensor return | 3G | ORN/BLK | 720 | Fuel Tank pressure sensor return
3H | DK GRN | 890 | Fuel tank pressure sensor signal | 3H | DK GRN | 890 | Fuel tank pressure sensor signal

#### In-Line Connector C405C/C405B

Connector Part Information |

• | 12146439

• | 4-Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12160830

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | 882 | RR wheel speed signal-high | A1 | BRN | 882 | RR wheel speed signal-high
B | WHT | 883 | RR wheel speed signal-low | B1 | WHT | 883 | RR wheel speed signal-low
C | BLK | 884 | LR wheel speed signal-high | C1 | BLK | 884 | LR wheel speed signal-high
D | WHT | 885 | LR wheel speed signal-low | D1 | WHT | 885 | LR wheel speed signal-low

#### In-Line Connector C405D/C405B

Connector Part Information |

• | 12162144

• | 4-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12160830

• | 16-Way Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | PNK | 239 | Fuse output-ignition 1--type III fuse | A2 | PNK | 239 | Fuse output-ignition 1--type III fuse
B | WHT | 1310 | Canister vent valve solenoid output | B2 | WHT | 1310 | Canister vent valve solenoid output
C-D | -- | -- | Not used | C2-D2 | -- | -- | Not used