For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 23907 Slide Hammer

• | J 26941 Extension Housing Seal Remover

1. Remove the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement in Propeller Shaft.
2. Remove the output shaft seal using J 23907 and J 26941 .

### Installation Procedure

#### Tools Required

J 21426 Extension Housing Seal Installer

1. Install the output shaft seal using J 21426 .
2. Lubricate the inside diameter of the seal with transmission fluid. Use Dexron® III transmission fluid or equivalent.
3. Install the propeller shaft. Refer to Two-Piece Propeller Shaft Replacement in Propeller Shaft.
4. Check the transmission fluid level. Refer to Transmission Fluid Level Inspection .