For 1990-2009 cars

1. Use feeler gauges to check the forward clutch plate travel. Check travel between the forward clutch backing plate retainer ring (651) and the forward clutch selective backing plate (650).

The forward clutch plate travel should be:

Specification

• | 245 mm -- 0.766-1.756 mm (0.030-0.069 in)

• | 298 mm/300 mm -- 0.866-1.876 mm (0.034-0.074 in)

2. Select the proper forward clutch selective backing plate (650) to obtain the correct travel. Refer to Forward Clutch Backing Plate Selection .