For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Exit the vehicle.
2. Close the door and the hatch.
3. Press the door UNLOCK button on the remote control door lock transmitter.

• | The driver door unlocks.

• | The interior lights illuminate.

• | Door Unlock Inoperative with Transmitter - All

• | Keyless Entry System Inoperative

• | Courtesy Lamps Inoperative with Transmitter

2 | Press the door UNLOCK button a second time within 5 seconds of the first press. |

• | The passenger door unlocks.

• | The interior lights stay illuminated for one of the following periods of time:

• | For 40 seconds after the first press of the UNLOCK button

• | Until the ignition switch is turned to the ON position

• | Door Unlock Inoperative with Transmitter - All

• | Door Lock/Unlock Inoperative - Right Side Front

• | Courtesy Lamps Inoperative with Transmitter

3 |

1. Wait for the interior lights to go out.
2. Press the door LOCK button on the remote control door lock transmitter.

• | The doors lock.

• | The interior lights illuminate for approximately 2 seconds in order to acknowledge the locking of the doors.

• | Door Lock Inoperative with Transmitter - All

• | Keyless Entry System Inoperative

• | Courtesy Lamps Inoperative with Transmitter

4 | Press the rear compartment lid release button on the remote control door lock transmitter. |

• | The rear compartment lid releases.

• | The interior lights illuminate for approximately 40 seconds.

• | Rear Release Inoperative with Transmitter

• | Keyless Entry System Inoperative

• | Courtesy Lamps Inoperative with Transmitter

5 | Enter the BCM feature customization mode. Refer to Feature Customization | BCM enters the feature customization mode. | RKE System Does Not Change Customization Modes