For 1990-2009 cars

# WATER LEAK THRU BOW LATCH INSTALL GROMMETS BOW LATCH PIN

#### SUBJECT: WATER LEAK INTO VEHICLE THRU #5 BOW LATCH (INSTALL 2 RUBBER GROMMETS ON #5 BOW LATCH PIN)

#### VEHICLES AFFECTED: 1989-91 CAMARO CONVERTIBLE

#### Application:

----------- 1989 - 1990 Chevrolet Camaro Convertible and 1991 prior to VIN ML165706

Condition: Inside of convertible top storage area may become wet.

Cause: Water enters stowage area through #5 bow latch.

Correction: Install TWO rubber grommets, P/N 12510756 on #5 bow latch pin as follows:

1. Open driver's side door and pull the #5 bow release latch forward.

2. Raise the #5 bow to full vertical position.

3. Install the rubber grommets on to the latch pin. The smaller diameter faces up for both grommets. Refer to Figure 1.

4. Lower and latch the #5 bow.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.