For 1990-2009 cars

Table 1: | Cruise Control Module
Table 2: | Stoplamp Switch (C1)
Table 3: | Cruise Control (Clutch) Switch
Table 4: | Cruise Control Release (Brake) Switch (Automatic Transmission)
Table 5: | Cruise Control Release (Brake) Switch (Manual Transmission)

#### Cruise Control Module

Connector Part Information |

• | 1206-5425

• | 10-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 397 | Cruise control on switch output
B | DK BLU | 84 | Cruise control set/coast switch signal
C | GRY/BLK | 87 | Cruise control resume/accel switch signal
D | BRN | 86 | Cruise control brake pedal switch input
E | BLK | 1650 | Ground
F | PNK | 139 | Fused ignition feed
G | LT BLU | 20 | Stop lamp switch input
H | DK GRN | 83 | Cruise control inhibit signal input
J | WHT | 85 | Cruise control status output
K | DK GRN/WHT | 817 | Vehicle speed sensor input

#### Stoplamp Switch (C1)

Connector Part Information |

• | 1203-3701

• | 2 Way F Metri-Pack 480 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 140 | Fused battery feed
B | LT BLU | 20 | Stoplamp switch output

#### Cruise Control (Clutch) Switch

Connector Part Information |

• | 1204-1433

• | 2 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 379 | Cruise control (clutch) switch output
B | PNK | 139 | Fused ignition feed

#### Cruise Control Release (Brake) Switch (Automatic Transmission)

Connector Part Information |

• | 1204-1433

• | 2 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 86 | Cruise control release (brake) switch output
B | PNK | 139 | Fused ignition feed

#### Cruise Control Release (Brake) Switch (Manual Transmission)

Connector Part Information |

• | 1204-1433

• | 2 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 86 | Cruise control release (brake) switch output
B | BRN/WHT | 379 | Cruise control (clutch) switch output