For 1990-2009 cars

# A/C R-12 CHARGING CAPACITIES ELIMINATE OVER & UNDER CHARGE

#### Models Affected: ALL 1985-90 PONTIAC VEHICLES

The following figure contains R-12 charging capacities for 1985 thru 1990 Pontiac vehicles. Keeping a copy in the area of the charging station should save time and eliminate conditions resulting from over or under charging.

PONTIAC R-12 CHARGING CAPACITIES

1985 1986 1987 1988 1989 1990

6000 2.75* 2.75* 2.75* 2.75* 2.75* 2.75

SUNBIRD 2.75 2.75 2.75 2.25 2.25 2.25

PARISIANNE/SAFARI 3.50 3.50 3.50 3.50 3.50 ----

LEMANS ---- ---- ---- 2.20 2.20 2.20

FIREBIRD 3.00 3.00 3.00 2.25 2.25 2.25

TRANSSPORT ---- ---- ---- ---- ---- 2.75

GRAND PRIX 3.25 3.25 3.25 2.25 2.25 2.25

FIERO 2.50 2.50 2.50 2.50 ---- ----

BONNEVILLE 3.25 3.25 2.40 2.40 2.40 2.40

T-1000 2.25 2.25 2.25 ---- ---- ----

GRAND AM 2.25 2.25 2.25 2.25 2.25 2.25

*STE - 2.25

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.