For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 8092 Driver Handle

• | J 34196-B Bushing Set

1. Remove the case rear oil seal (106) (Y-car Only).
2. Remove the case bushing (7) using J 8092 and J 34196-B .

### Installation Procedure

#### Tools Required

• | J 8092 Driver Handle

• | J 34196-B Bushing Set

• | J 42198 Case Rear Oil Seal Installer

1. Install a case bushing (7) using J 8092 and J 34196-B .
2. Install a case rear oil seal (106) (Y-car Only) using J 42198 .