For 1990-2009 cars

# LTG. REQUEST FOR REVIEW CHANGE SEPTEMBER-novEMBER

This bulletin addresses changes to the published Pontiac Labor Time Guide; September and November changes are attached. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future 1988 Labor Time Guide revisions. In the case of past model year updates, it is recommended that this bulletin be retained with all appropriate model year Labor Time Guides, as a complete revision will not be provided.

#### REQUEST FOR REVIEW

OPERATION DESCRIPTION OPERATION VEHICLE SERIES NUMBER A B F G H J N P T VIN CODE

PANEL/CARRIER ASSEMBLY, INSTRUMENT CONTROL C2549 5.3 -REPLACE NOTE: Applicable model years: 1986-1987

BLADDER ASSEMBLY, PNEUMATIC SEAT - REPLACE LUMBAR SEAT BACK PASSENGER C7070 .4 DRIVER C7071 .4 NOTE: Applicable model years: 1987-1988

BRACKET, POWER STEERING PUMP ASSEMBLY, MOUNTING E9020 .6 -REPLACE NOTE: Applicable model years: 1987-1988 with 2.8L V-6. ADD: A-With A/C .1 B- To Replace Front Mounting Bracket .2

BOOSTER ASSEMBLY, H1300 1.0 HYDRAULIC POWER BRAKE - R&R NOTE: Applicable model year: 1985

SEAL(S) CRANKSHAFT J1120 3.5 REAR MAIN - REPLACE NOTE: Applicable model years: 1981-87 w/ auto trans (T 1000). ADD: A- With P/S 1

TENSIONER, SERPENTINE J0680 BELT - REPLACE NOTE: Applicable model years: 1987-88 (Correction to the misprint in the MAY/JUNE Bulletin.) L4 .7 V-6 .2

BELT, DRIVE - ADJUST NOTE: Applicable model year: 1987 w/ 2.8L ONE J0656 .3 ALL J0657 .4

BELT, DRIVE - REPLACE NOTE: Applicable model year: 1987 w/ 2.8L A/C J0660 .5 FAN/GENERATOR J0663 .3

CAP, RADIATOR FILLER J3020 .5 - REPLACE NOTE: Applicable model years: 1987-1988

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

SWITCH - REPLACE

SEAT LUMBAR CONTROL ADJUST LEFT N2417 .2 NOTE: Applicable model years: 1987-1988

RELAY - REPLACE SEATBACK BLADDER MOTOR N2898 .6 NOTE: Applicable model years: 1987-1988

INSTRUMENT PANEL CLUSTER COMPONENTS (DIGITAL/ELECTRONIC) NOTE: Applicable model years: 1986-1988 ODOMETER AND/OR N4192 .5 ODOMETER MOTOR

VALVE, SEATBACK BLADDER N3480 .6 -REPLACE NOTE: Applicable model years: 1987-1988

MODULE - REPLACE NOTE: Applicable model years: 1987-1988 HEADLAMP CLOSURE PANEL N4829 RIGHT .3 LEFT .3

MEMORY SEAT SYSTEM COMPONENTS - REPLACE MODULE N5510 .5 .5 SWITCH N5520 .2 .2 NOTE: Applicable model years 1987-1988

FIBER OPTIC, ILLUMINATED DOOR LOCK - REPLACE NOTE: Applicable model years: 1987-1988 RIGHT R4440 .5 LEFT R4441 .5

TRANSPORTATION CLAIM OPERATIONS LOOSE SHIPPED ITEMS S0014 .2 .2 .2 .2 .2 .2 .2 .2 .2 -REPLACE NOTE Applicable model YEARS: All

#### REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

RESERVOIR, RADIATOR J3260 .5 COOLANT - REPLACE NOTE: Applicable model years: 1987-1988 ADD: A- With A/C .1

GENERATOR ASSEMBLY J4100 1.3 - REPLACE NOTE: Applicable model years: 1987-88 W/ 2.5L

SENSOR, CAMSHAFT J4350 .6 -REPLACE NOTE: Applicable model year: 1987

SOLENOID, STARTER J4580 1.1 MOTOR - REPLACE NOTE: Applicable model years: 1984-85 ADD: A-With A/C .1

DRIVE ASSEMBLY, J4600 .8 STARTER MOTOR - REPLACE NOTE: Applicable model years: 1984-88 'A' series W/ 2.5L; 1984-85 'T' series. ADD: A-With A/C .1

MOTOR ASSEMBLY, J4620 .6 1.1 STARTER - R&R NOTE: Applicable model years: 1984-88 'A' series w/ 2.5L; 1985-85 'T' series. ADD: A-With A/C .1

MOTOR ASSEMBLY, J4640 .6 1.1 STARTER - REPLACE NOTE: Applicable model years: 1984-88 'A' series w/ 2.5L; 1984-85 'T' series. ADD: A-With A/C .1

CYLINDER, CLUTCH K0600 .8 MASTER - R&R OR REPLACE NOTE: Applicable model years: 1987-1988 (Correction to the misprint in the JULY/AUGUST Builetin.)

CLUTCH SYSTEM,HYDRAULIC K0040 .5 - BLEED NOTE: Applicable model years: ALL

SWITCH - REPLACE SEAT LUMBAR CONTROL ADJUST RIGHT N2416 .2

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.