For 1990-2009 cars

### Removal Procedure

The roof lift-off window is adjustable within the lift-off window opening. The roof lift-off windows are adjusted up and down by adding or removing backing plates (4). Inboard/outboard and fore-and-aft travel is adjusted by loosening bolts/screws (2) and repositioning the front and rear strikers (1 & 3) as necessary. Adjustments should be made to get a flush fit of the roof lift-off window to the roof.

1. Remove roof lift-off window. Refer to Lift-Out Panel Replacement .
2. Remove windshield side upper garnish molding.
3. Remove quarter trim finish panel bolts/screws.
4. Remove quarter inner trim finish panel extension to access rear striker (3).
5. Loosen bolts/screws (2).

### Installation Procedure

1. Install quarter inner trim finish panel extension.
2. Install quarter trim finish panel bolts/screws.

Tighten
Tighten the quarter trim finish panel bolts/screws to 1.7 N·m (15 lb in).

3. Install windshield side upper garnish molding.
4. Install roof lift-off window. Refer to Lift-Out Panel Replacement .