For 1990-2009 cars

#### Tools Required

• | J 5825-A Crankshaft Sprocket Puller

• | J 39243 Water Pump Driveshaft Remover

1. Remove the crankshaft position sensor reluctor ring.
2. Remove the camshaft sprocket bolts.
3. Remove the camshaft sprocket.
4. Remove the timing chain.
5. Remove the crankshaft sprocket.
6. If necessary, remove the crankshaft sprocket key.
7. Use the J 39243 in order to remove the water pump driveshaft.