For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
2. Disconnect the accelerator cable (3) from the accelerator pedal lever (2).
3. Squeeze the accelerator cable cover tangs (1) and push the cable through the dash panel.
4. Disconnect the accelerator cable from the intake manifold bracket.
5. Remove the accelerator cable from the slot in the accelerator cable bracket.
6. Disconnect the accelerator cable from the throttle body lever.
7. Remove the accelerator cable.

### Installation Procedure

1. Install the accelerator cable (3) through the dash panel. Snap the retainer (1) through the dash panel.
2. Install the accelerator cable (3) through the slot in the accelerator pedal lever (2). Seat the retainer (4) in the accelerator pedal lever (2).
3. Connect the accelerator cable to the throttle body lever.
4. Slide the accelerator cable into the slot on the accelerator cable bracket. Snap the locking tab into position.
5. Connect the accelerator cable to the intake manifold bracket.
6. Check for complete throttle opening and closing positions by operating the accelerator pedal. Also check for poor carpet fit under the accelerator pedal. The throttle should operate freely without bind between full closed throttle and wide open throttle.
7. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.