For 1990-2009 cars

### Circuit Description

The PCM performs an internal self-test on it's Random Access Memory (RAM) or read/write memory. If this self-test fails, this DTC sets.

### Conditions for Running the DTC

• | The ignition voltage is greater than 10 volts.

• | The ignition is ON for 5 seconds.

### Conditions for Setting the DTC

The internal RAM test fails.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) when the diagnostic runs and fails.

• | The PCM records the operating conditions at the time the diagnostic fails. The PCM stores this information in the Freeze Frame and/or Failure Records.

### Conditions for Clearing the MIL/DTC

Replace the PCM.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This DTC indicates an internal PCM condition.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | Important:: Program the replacement PCM. Refer to Powertrain Control Module Replacement/Programming . Replace the PCM. Is the action complete? | -- | Go to Step 3 | --
3 |

1. Select the Diagnostic Trouble Code (DTC) option and the Clear DTC option using the scan tool.
2. Idle the engine at the normal operating temperature.
3. Select the Diagnostic Trouble Code (DTC) option and the Specific DTC option, then enter the DTC number using the scan tool.
4. Operate vehicle within the Conditions for Running the DTC as specified in the supporting text, if applicable.

Does the scan tool indicate that this test ran and passed?

--

Go to Step 4

Go to Step 2

4 | Select the Capture Info option and the Review Info option using the scan tool. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to applicable DTC table | System OK