For 1990-2009 cars

Clean the following components of the tape player after every 50 hours of cassette operation:

• | The head

• | The capstan

Leave the radio in the vehicle when you clean the above components. You can access the components through the tape door.

Use one of the following items in order to clean the head and the capstan:

• | A cotton swab dipped in rubbing alcohol

• | A cassette cleaning kit

| Follow the instructions with the kit to clean the tape player.

Do not contact the tape head with magnetized tools. If the head becomes magnetized, it will degrade every cassette tape played in the tape player.

The tape deck has an added function that helps prevent damage if the cassette tape breaks or becomes jammed. The tape deck may eject the scrubbing-type, cleaning cartridge after about 5 seconds. Therefore, insert the scrubbing-type cleaner at least 3 times in order to clean the deck thoroughly.

A non-scrubbing, wet type tape cleaner can be used in place of the scrubbing type. The non-scrubbing, wet type uses a fabric belt in place of the tape and will not eject after 5 seconds. However, the non-scrubbing, wet type tape cleaner may not provide a thorough cleaning, such as the scrubbing type cleaner.

No service is provided on tape cassettes. The cassette manufacturer handles the warranties of the cassettes. The test cassette used by the dealer should be stored in its container in order to remain clean. Store the cassettes away from extreme heat and direct sunlight.