For 1990-2009 cars

### Removal Procedure

1. Raise rear compartment lift window.
2. Remove sunshade by unsnapping from installed position.
3. Remove three retainers by rotating retainers a quarter turn using a key or coin if removing right quarter inner rear trim finishing panels.
4. Begin removing quarter inner rear trim finishing panels (1) by first lifting from front corner.
5. Completely remove quarter inner rear trim panels (1) by lifting the front of the panels, gently unseating the remaining retainers (left side removal only).
6. Remove speaker electrical connections (3) from speakers (4).
7. Remove speaker grille if replacing panel.
8. Remove rear speakers from panels.
9. Remove and save retainers on left panel for reuse if replacing panel.

### Installation Procedure

1. Install three retainers to new panels if replaced.
2. Install rear speakers to panels if panels were removed.
3. Install speaker grille if removed.
4. Install speaker electrical connections (3) to speakers (4).

Important: On left panel, align the three retainers with the holes in the body and press down firmly to engage clips. Ensure that clips "click" into place.

5. Install quarter inner rear trim finishing panel.
6. Seat the three retainers by rotating retainers a quarter turn using a key or a coin if installing left panel.
7. Install sunshade by snapping into position.
8. Lower rear rear compartment lift window.