For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the vehicle with safety stands.
3. Support the transmission with a transmission stand.
4. Remove the transmission mount nut (2).
5. Remove the transmission support bolts (2).
6. Remove the transmission support (1).
7. Remove the transmission mount bolts.
8. Remove the transmission mount.

### Installation Procedure

1. Install the transmission mount.
2. Install the transmission mount bolts

Tighten
Tighten the transmission mount bolts to 48 N·m (36 lb ft).

3. Install the transmission support (1).
4. Install the transmission support bolts (2).

Tighten
Tighten the transmission support bolts (2) to 57 N·m (43 lb ft).

5. Install the transmission mount nut (2).

Tighten
Tighten the transmission mount nut (2) to 57 N·m (43 lb ft).

6. Remove the support from the transmission.
7. Remove the vehicle safety stands.
8. Lower the vehicle.