For 1990-2009 cars

#### Definitions

The following are symptomatic noises of the accessory drive belt system:

1. Chirping:

• | A high pitched noise that is usually heard once per revolution of a pulley or a belt.

• | It is most common on cold, damp mornings.

• | Verify this condition by squirting water onto the belt. The noise will momentarily stop.

2. Squeal:

• | A loud screeching noise that is caused by a slipping belt (this is unusual for a multiple ribbed belt).

• | The noise occurs when a heavy load is applied to the belt, such as an air conditioning compressor engagement, snapping the throttle, or slipping on a seized pulley.

3. Knocking:

• | A low pitch tapping noise caused by belt misalignment.

• | This noise occurs on cold start-up at idle.

4. Whine: A high pitched continuous noise that may be caused by a failed component bearing.
5. Faint Cycle Rumbling: A low frequency noise heard once per revolution of the belt.
6. Pilling:

• | The random accumulation of rubber dust in the bottom of the multi-ribbed belt grooves.

• | A small amount of pilling is normal.

• | Operation of the drive belt system will not be effected unless the buildup exceeds one third (1/3) of the belt groove depth.

Multiple ribbed, accessory drive belts wear evenly with their pulleys. Unusual wear indicates a correction is needed. The following diagnostic tables will aid in diagnosing drive belt system problems.