For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Using a test light, backprobe between C216 terminal P and ground.
2. Depress and hold the brake pedal.

Does the test light illuminate?

--

Go to Step 3

Go to Step 4

3 | Replace the turn/hazard switch assembly. Refer to Hazard Warning Switch Replacement . Is the repair complete? | -- | Go to Step 5 | --
4 | Repair a poor connection or open in circuit 20. Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all repairs been made?

--

Go to Exterior Lights System Check

--