For 1990-2009 cars

# RTV SEALANT REPLACEMENT REPAIR VALVE COVER OIL LEAKS

1980-84 PHOENIX, FIREBIRD, AND 6000

A new composition gasket, P/N 14089252, is available for service use on all 2.8L V6 engines.

This gasket replaces the RTV sealant and is to be used for repair of rocker arm cover oil leaks and general service work.

A small amount (DAB) of GM sealer must be applied at the cylinder head - intake manifold split line prior to the gasket installation.

The rocker arm cover attaching bolts must be torqued to 8.5 to 10 N.m (75-90 in. lb.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.