For 1990-2009 cars

# CLUTCH PEDAL CONTACT HUSH PNL. TRIM EDGE OF HUSH PANEL

#### SUBJECT: HUSH PANEL REWORK - CONTACT WITH CLUTCH PEDAL (TRIM HUSH PANEL FROM EDGE)

#### VEHICLES AFFECTED: 1990-91 F-CARS WITH STANDARD TRANSMISSION

#### Condition:

--------- Some owners may comment that the clutch pedal contacts the edge of hush panel.

#### Cause:

----- Hush panel and or clutch pedal slightly mispositioned due to build variation.

#### Correction:

---------- Remove left side (driver side) hush panel. Using a sharp cutting tool trim off approximately 3 mm (1/8 inch) material from edge of hush panel where clutch makes contact. (See Illustration).

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.