For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Remove the instrument panel driver knee bolster. Refer to Instrument Panel Driver Knee Bolster Replacement in Instrument Panel, Gauges, and Console.
3. Disconnect the clutch anticipate switch harness electrical connector from the clutch anticipate switch.
4. Disconnect the clutch anticipate switch from the brake and accelerator and the clutch pedal (with bracket).

### Installation Procedure

1. Connect the clutch anticipate switch to the brake and accelerator and clutch pedal (with bracket).
2. Connect the clutch anticipate switch harness electrical connector to the clutch anticipate switch.
3. Install the instrument panel driver knee bolster. Refer to Instrument Panel Driver Knee Bolster Replacement in Instrument Panel, Gauges, and Console.
4. Connect the negative battery cable.