For 1990-2009 cars

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement in Engine Electrical.
2. Remove the coolant recovery reservoir hose from the radiator.
3. Remove the accelerator and cruise control servo cable bolts, if equipped.
4. Reposition the accelerator and cruise control servo cable adjuster, if equipped.
5. Remove the coolant recovery reservoir bolt.
6. Remove the wiring harness rosebud clip from the reservoir neck.
7. Remove the coolant recovery reservoir.
8. Remove the coolant recovery reservoir hose and grommet from the reservoir.
9. Clean the coolant recovery reservoir with soap and water. Thoroughly rinse the reservoir.

### Installation Procedure

1. Install the coolant recovery reservoir hose and grommet to the reservoir.
2. Install the coolant recovery reservoir.
3. Install the wiring harness rosebud clip to the reservoir neck.
4. Install the coolant recovery reservoir bolt.

Tighten
Tighten the coolant recovery reservoir bolt to 12 N·m (106 lb in).

5. Position the accelerator and cruise control servo cable adjuster, if equipped.
6. Install the accelerator and cruise control servo cable bolts, if equipped.

Tighten
Tighten the servo cable adjuster bolts to 7.5 N·m (66 lb in).

7. Install the coolant recovery reservoir hose to the radiator.
8. Install the battery. Refer to Battery Replacement in Engine Electrical.
9. Add engine coolant to the FULL COLD mark on the reservoir.