For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Using a scan tool, command the powertrain control module (PCM) to deflect the fuel gage to half full. Does the fuel gage read half full? | -- | Go to OBD II Diagnostic System Check | Go to Step 2
2 |

1. Inspect CKT 1936 between the instrument cluster and the PCM for an open or poor connection.
2. If CKT 1936 is OK, replace the cluster. Refer to Instrument Cluster Replacement .

Did you complete the repair?

--

System OK

--