For 1990-2009 cars

### Removal Procedure

1. Disconnect the three vacuum hoses from the evaporative emission (EVAP) canister.
2. Remove the two bolts from the EVAP canister bracket.
3. Remove the EVAP canister and bracket from the bulkhead.

### Installation Procedure

1. Install the EVAP canister and bracket to the bulkhead.
2. Secure the EVAP canister bracket with the two bolts.

Important: Refer to the Vehicle Emissions Control Information Label for the proper routing of the EVAP hoses.

3. Connect the three vacuum hoses to the EVAP canister.