For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Daytime Running Lamps (DRL) Check? | -- | Go to Step 2 | Go to Daytime Running Lights (DRL) System Check .
2 |

1. Turn the combination switch to the HEAD position.
2. Move the dimmer switch in the HI position.
3. Using J 35616-200 , backprobe the junction block connector C3 from cavity 6 to B+.

Does the test lamp light?

--

Go to Step 3

Go to Step 5

3 | Inspect for an open in the RED wire between S107 and the junction block. Is the connection OK? | -- | Go to Step 4 | Go to Step 6
4 | Replace the junction block. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check . | --
5 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check . | --
6 | Repair the open in the RED wire between S107 and the junction block. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check . | --