For 1990-2009 cars

1. Adjust the rear toe by loosening/tightening both body-side (cam) control rod nuts (3) and bolts (2).
2. Loosen the right and left body-side control rod nuts (3).
3. Loosen the right and left body-side control rod bolts (cam bolts) (2) by the same amount.
4. Set the rear total toe to 0.3 to 0.6 degrees.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Hold the control rod bolt with a wrench to prevent it from turning while tightening the control rod nuts.

5. Tighten the left and right body-side control rod nuts.

Tighten
Tighten the left and right body-side control rod nuts to 80 N·m (59 lb ft).