For 1990-2009 cars

### Removal Procedure

1. Disconnect the following connectors from the radio by accessing through the instrument panel compartment:

• | The radio electrical connector

• | The antenna connector

2. Remove the ashtray from the track by pushing down on the retainer and pulling out.
3. Remove the following components from the instrument panel:

3.1. | 4 screws (1)

3.2. | The center trim bezel (3)

4. Remove the cross-recess screw (1) from under the back of the radio. Access the screw through the ashtray cutout in the instrument panel.
5. Remove 4 screws from the front of the radio.
6. Remove the radio with the mounting bracket from the vehicle.
7. Remove 5 screws and 3 radio mounting brackets from the radio, if necessary.

### Installation Procedure

1. Install the radio mounting brackets to the radio, if removed. Secure the brackets with the 5 screws.
2. Install the radio to the instrument panel. Secure the radio with 4 screws (1).
3. Install the cross-recess screw to the radio rear mounting bracket. Access through the ashtray cutout in the instrument panel.
4. Install the center trim bezel (3) to the instrument panel. Secure the bezel with the 4 screws (1).
5. Install the ashtray to the ashtray track.
6. Connect the following connectors. Access through the instrument panel compartment:

• | The radio electrical connector

• | The antenna connector