For 1990-2009 cars

### Removal Procedure

Important: Observe the location of the wiper arm (2) before you remove the wiper arm. This will ensure correct installation.

1. Remove the nut cover and the retaining nut from the wiper arm.
2. Remove the wiper arm (2) from the wiper linkage (3).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the wiper arm (2) to the wiper linkage (3). Secure the wiper arm with the retaining nut.

Tighten
Tighten the wiper arm retaining nut to 20 N·m (15 lb ft).

2. Install the wiper arm nut cover to the wiper arm.