For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the ON position.
2. Pull the front wiper/washer switch lever.

• | The front washer pump operates.

• | The wipers operate at LOW speed.

• | Washers Inoperative

• | Wipers All Modes and Washer Inoperative

2 | Release the wiper/washer switch. |

• | The front washer pump stops.

• | The wipers complete the cycle and return to the PARK position.

Wipers Blades Do Not Park

3 | Move the front wiper/washer switch lever to the LO position. | The wipers operate at LOW speed. | Wipers High Mode Operates with Switch in Low
4 | Move the front wiper/washer switch lever to the HI position. | The wipers operate at HIGH speed. |

• | Wipers Low Mode Operates with Switch in High

• | Wipers High Mode Inoperative

5 | Move the front wiper/washer lever to the INT position. | The wipers sweep once every 6 seconds. | Wipers Delay Mode Inoperative
6 | Move the front wiper/washer switch lever to the OFF position. | The wipers complete the cycle and return to the PARK position. |

• | Wipers Blades Do Not Park

• | Wipers Always On

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.