For 1990-2009 cars

### Removal Procedure

1. Discharge and recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the air cleaner from the vehicle.
3. Remove the A/C refrigerant pressure switch from the evaporator inlet tube. Refer to Pressure Cycling Switch Replacement .
4. Remove the evaporator inlet tube at the bulkhead fitting (2).
5. Disconnect the evaporator inlet from the receiver-dryer outlet pipe fitting (7) in front of the condenser fan.
6. Remove the evaporator inlet tube from the inner fender retaining clip.
7. Remove the evaporator inlet tube from the vehicle.

### Installation Procedure

1. Lubricate new O-rings with mineral base 525 viscosity refrigerant oil.
2. Install the O-rings to the evaporator inlet pipe.
3. Install the evaporator inlet tube to the vehicle. Secure the evaporator inlet tube at the inner fender retaining clip.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Connect the evaporator inlet to the receiver-dryer outlet pipe fitting (7).

Tighten
Tighten the pipe fitting to 35 N·m (26 lb ft)

5. Connect the evaporator inlet tube at the bulkhead fitting (2).

Tighten
Tighten the pipe fitting to 35 N·m (26 lb ft)

6. Install the A/C refrigerant pressure switch to the evaporator inlet pipe. Refer to Pressure Cycling Switch Replacement .
7. Install the air cleaner to the vehicle.
8. Evacuate and recharge the A/C system. Refer to Refrigerant Recovery and Recharging .
9. Operate the A/C system, and test the system for refrigerant leaks. Refer to Leak Testing .