For 1990-2009 cars

### Removal Procedure

Notice: When replacing a speedometer or odometer assembly, federal law requires that the odometer reading of the replacement unit be set to register the same mileage as the prior odometer. If the same mileage cannot be set, the law requires that the replacement odometer be set at zero and a label be installed on the driver's door frame to show the previous reading and the date of replacement.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster from the instrument panel. Refer to Instrument Cluster Replacement .
3. Push on the tabs in order to remove the cluster lens (7) and the bezel assembly (6) from the cluster housing.
4. Remove 4 screws (2) that secure the speedometer to the cluster housing.
5. Remove the speedometer gauge (5) from the cluster housing (3).

### Installation Procedure

1. Install the speedometer gauge (5) to the cluster housing (3).
2. Secure the speedometer gauge to the cluster housing with 4 screws (2).
3. Install the cluster lens (7) and the bezel (6) to the cluster housing (3).
4. Install the instrument cluster to the instrument panel. Refer to Instrument Cluster Replacement .
5. Connect the negative battery cable.