For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Daytime Running Lamps (DRL) Check? | -- | Go to Step 2 | Go to Daytime Running Lights (DRL) System Check
2 |

1. Turn the ignition switch to the ON position.
2. Using a fused jumper, backprobe the IP cluster assembly connector C3 from cavity 2 to ground.

Does the DRL indicator light?

--

Go to Step 3

Go to Step 5

3 | Inspect for an open in the ORN/WHT wire between the instrument panel cluster assembly and the DRL control module. Is the connection OK? | -- | Go to Step 4 | Go to Step 6
4 | Replace the DRL control module. Refer to Daytime Running Lights (DRL) Control Module Replacement . Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check | --
5 | Repair or replace the printed circuit of the instrument panel cluster. Refer to Printed Instrument Cluster Circuit Replacement in Instrument Cluster. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check | --
6 | Repair the open in the ORN/WHT wire between the instrument panel cluster assembly and the DRL control module. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check | --